**Albus Security**

**Practical Challenge – 6**

**Approach:** To solve the task, I will review the Spanning tree configuration and assign priority to the switches

**Solution:**

Admin Switch: -

* **conf t**
* **spanning-tree vlan 1 priority 4096**
* **show spanning-tree**

Junior Switch: -

* **conf t**
* **spanning-tree vlan 1 priority 8193**
* **show spanning-tree**

Senior Switch: -

* **conf t**
* **spanning-tree vlan 1 priority 12288**
* **show spanning-tree**